Search Tips

Search is based on keyword.

`Ex: "Procedures"`

Do not search with natural language

`Ex: "How do I write a new procedure?"`

Give Feedback Support Portal

# OCIODisplay

This node is used to convert the input colorspace to display device-suitable values.

Connection Type | Connection Name | Function
Input | input | The place in the node graph where the colorspace conversion is applied.

Control (UI) | Default Value | Function
inputColorSpace | linear | Sets the input colorspace to convert from.
display | sRGB | Sets the output display colorspace to convert to.
view | sRGB | Specifies the colorspace transform to apply to the scene or image, from the options Film, Log, or Raw.
exposure
rgb | 0 | Sets the exposure level for the r, g, and b channels together.
r | 0 | Sets the exposure level for the red channel.
g | 0 | Sets the exposure level for the green channel.
b | 0 | Sets the exposure level for the blue channel.
context Manually define keys and values for the OCIODisplay node.
key1; key2; key3; key4 | N/A | Set a key that corresponds to the value of the same number in order to modify elements of the OCIO node, for example, setting a key called SHOT now tells the node that the corresponding value should be used for shots.
value1; value2; value3; value4 | N/A | Set a value that corresponds to the key of the same number in order to modify elements of the OCIO node, for example, setting a value fora key called SHOT now tells the node that this value should be used in this context.